GREEN LASER SIGHT 
ITEM: COVERT GREEN
INSTRUCTIONS
This laser sight is engineered for direct mounting onto your firearm's Picatinny rail. While it is not intended to replace primary sighting devices for precision accuracy, this unit will significantly assist in quickly acquiring your target. It can be easily mounted on any Picatinny configuration you select. 

WARNING:

Before handling the unit, read and understand the contents of this manual.

·NEVER point the illuminator directly at, or into, an eye. This may cause damage to the eye or blindness. The illuminator produces enough light to identify an individual without direct illumination to the face.

·Avoid looking directly into the illuminator’s beam.

·Avoid shining the illuminator into mirrors or other reflective surfaces.

·Avoid hitting or dropping the unit.

·The illuminator should be tested during periods of non-use to make sure it is still operating properly.

·NEVER allow children to use or handle this product.

·CAUTION: Use of controls or adjustments or performance of procedures other than those specified herein may result in hazardous radiation exposure.

Failure to follow the above warnings is dangerous and may result in serious injury or damage to property.
DANGER: AVOID DIRECT EYE EXPOSURE TO LASER BEAM. LASER RADIATION IS EMITTED FROM THE APERTURE.
Note: If you are not sure about any of the procedures in this manual, please seek the help of a qualified professional to avoid the damage of your laser sight and your firearm.

CAUTION: BEFORE INSTALLATION OF YOUR LASER SIGHT, BE SURE THAT THE RIFLE IS UNLOADED. ALWAYS PRACTICE SAFE RIFLE HANDLING PROCEDURES.

Statement:

The product has been carefully checked and tested in our factory, please check carefully Before using the product, inspect it for any damage that may have occurred during transport and confirm that all accessories are included. The accessories include: 1. Type-c Recharge wire; 2. Remote wire pressure switch. 3. 1.5mm Allen wrench; 4. 2.5mm Allen wrench; 5. Instruction manual
Note: Always be sure to recharge this laser sight after use to avoid draining the battery. Please charge this product once every three months and fully charge it before storing it for the first time.
Maintenance:
If the beam quality degrades due to dust, vapor, or smoke, the optical port's lens should be gently wiped immediately with a clean, soft cloth or lens cleaning paper.

To prevent the degradation of light quality, do not wipe the lens with solvents unless instructed by a professional
Specifications: 
·Model: COVERT GREEN
·Brand Name: Osprey Global
·Output Power: <5mW  

·Wavelength: 520nm

·Class IIIA Laser Product

·Voltage: 5VDC max input (USB Output application)
·Source Type: Rechargeable Battery (ICR10280)

·Working Temperature: -20℃ ~ +60℃

·Storage Temperature: -20℃ ~ +60℃ 

·Three modes: 

Green laser is always on;

Green laser is flashing;

Green laser is off.

·Battery Life: Approximately 3hrs (Continuous use)

·Body Material: Black Aluminum Alloy

·Switch: Digital Button and remote wire pressure switch;
·Weight: 1.6oz (Battery Incl.)

·Size(inch): 3(L)*1.1(W)*0.8(H)

·Warranty: Lifetime
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        Figure 1

Instruction for Figure 1:

(1) Laser sight

(2) Windage Adjustment Screw

(3) Elevation Adjustment Screw  

(4) Laser beam’s aperture

(5) Clamp screw of mount
(6) Clamp

(7) Port for remote wire pressure switch

(8) Digital On/Off button 
(9) Type-c Charging Port (DC5V application)
(10) Type-c cable

(11) Remote wire pressure switch
Operation:

Mounting Instructions
The unit features a built-in mount designed to fit a standard Picatinny rail.

Loosen the screw (5).

Slide the laser onto the rail at the desired position.

Fasten the screw, but do not over-tighten it.

Charging Instructions

This unit includes one Type-C charging cable.

Ensure the charger is fully connected to the charging port on the laser body.

The LED will turn solid red during charging.

When fully charged, the red LED will turn off.

Note: The battery is fully charged from the factory. The LED may turn off quickly upon initial charging. If the USB output voltage from your computer or power adapter is low, the Red LED may not turn off when charging is complete, but the battery will be fully charged within a maximum of 2 hours. 

Use switches:

Standard Momentary ON/OFF Button:

Pressing the button (8) cycles the laser through its modes in the following sequence: OFF → ON  → Flash → OFF.

Remote Wire Pressure Switch:

To use the remote switch, insert its plug into the jack on the body (7). The laser will turn ON only while the remote wire pressure switch pad (11) is being depressed and will turn OFF immediately upon release.

Zeroing:

Use supplied Allen wrench to adjust the windage and elevation.

SPECIAL NOTE: THIS UNIT WILL ONLY WORK UNDER THE TEMPERATURES LISTED ABOVE. THE UNIT WILL NOT WORK IN EXTREME COLD OR EXTREME HEAT. 

CAUTION - LASER LIGHT IS BRIGHT AND BLINDING - DO NOT SHINE AT AIRCRAFT OR VEHICLES AT ANY DISTANCE.
Replacing the battery:
The rechargeable battery has an approximate lifespan of 500 to 1,000 charge cycles. To replace it, unscrew the three screws located on the bottom of the unit, insert the new rechargeable battery, and then securely tighten the screws.

Note: If you are not sure of any of the procedures in this manual, always seek the help of a qualified professional to avoid damage to your laser device and your firearm.
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